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How to connect the AF PLC to the PC
For your technical question, we would like to answer as below,
1) Pls kindly install the USB driver firstly, the name is FTD232.
2) Under Windows 7, you need to select the QUICKII property, and select "Windows XP compatibility " to run QUICKII.
3) You could check COM port through your Device Manager to choose the correct COM.
4) For PLC, you must power on.
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